Concrete Finisher (Water main and Sewer Construction) (NOC: 7282)

**Employer:** CKB Construction

**Website**: [http://www.ckbconstruction.com](http://www.ckbconstruction.com/)

**Title:** Concrete Finisher (Water main and Sewer Construction) (NOC: 7282)

12 vacancies

**Terms:**

Seasonal, Full Time, Day, Evening, Weekend, Overtime

**Salary**: $31.50.00 to $33.00 Hourly, based on experience

**Benefits**: Dental Benefits, Short-Term Disability Benefits, Extended Medical Benefits, Life Insurance Benefits, Vision Care Benefits, RRSP Matching. Referral and Performances Bonuses available.

**Hours**: 32 to 44 Hours per week, depending on weather

**Anticipated Start Date**: Spring 2020 (actual start date is weather-dependent)

**Work Location**: Various locations in Alberta (travel expenses and living out allowance covered as per company policy)

**Work Site Environment:** Dusty, Noisy, Outdoors, Underground

**Requirements:**

**Education:** Not required  
  
**Experience:** 3 years of relevant experience  
  
**Languages:** English

**Security and Safety:** Pre-access drug and alcohol screening required prior to working on specific locations

**Own Tools/Equipment:** Steel-toed safety boots

**Work Conditions and Physical Capabilities:** Physically demanding, Handling heavy loads (Up to 45 kg/100 lbs), Bending, crouching, kneeling, Attention to detail, Standing for extended periods

**Personal Suitability:** Team player, Flexibility, Organized  
  
**Skills:**

* Check formwork, granular base and steel reinforcement materials and direct placement of concrete into forms or onto surfaces according to grade
* Fill hollows and remove spots on freshly poured cement
* Operate power vibrators to compact concrete
* Level top surface concrete according to grade and depth specification
* Impart desired finish to concrete surfaces using hand and power tools
* Install anchor bolts, steel plates
* Repair, resurface and replace worn or damaged sections of concrete structures
* Level earth to fine grade specifications
* May assist in aligning pipes during pipeline construction (water main and sewer construction)
* Set and install concrete structures
* Place and finish concrete within and around concrete structures (manholes, storm management structures)
* Placing and finishing of concrete sidewalk and curb and gutter
* Must be able to access and egress trenches.

**Type of Construction:** Water main and Sewer Construction, Sidewalks and curb and gutter

**Type of Materials:** Reinforcing membrane and protective covering

**How to Apply:**

**By Mail:**

10828-209 Street  
Edmonton, Alberta  
T5S 1Z9

**By E-mail:**

[Concrete@ckbconstruction.com](mailto:Concrete@ckbconstruction.com)